|  |  |  |  |
| --- | --- | --- | --- |
| **STEP** | **COMMANDER** | **PROCEDURE** | **CONDITION** |
| 1 | MCCC | SURFACE WARNING CONTROL  | Indicator Red  |
| 2 | MCCC & DMCCC | LAUNCH KEYS . . . . . . . . . . . . . .  | Inserted |
| 3 | BMAT | CIRCUIT BREAKER 101 ON . . . .  | Set |
| 4 | BMAT & MFT | BVLC - OPERATE CODE WORD  | Entered |
| 5 | BMAT & MFT | BVLC - OPERATE SWITCH . . . . . . . .  | Activated |
| 6 | BMAT | OPERATE INITIATE . . . . . . . . . . .  | Indicator On |
| 7 | BMAT | OPERATE OK . . . . . . . . . . . . . . .  | Indicator On |
| 8 | MCCC & DMCCC | LAUNCH KEYS, AT COMMIT TIME . . . . . . . . . . . . . . . . . . . . . . .  | Turned, Held |
| 9 | MCCC | LAUNCH ENABLE . . . . . . . . . . . .  | Indicator On |
| 10 | MCCC | BATTERIES ACTIVATED . . . . . .  | Indicator On |
| 11 | MCCC | APS POWER . . . . . . . . . . . . . . . . | Indicator On |
| 12 | MCCC | SILO SOFT . . . . . . . . . . . . . . . . . . | Indicator On |
| 13 | MCCC | GUIDANCE GO . . . . . . . . . . . . . .  | Indicator On |
| 14 | MCCC | FIRE ENGINE . . . . . . . . . . . . . . . .  | Indicator On |
| 15 | MCCC | LIFT-OFF . . . . . . . . . . . . . . . . . . .  | Indicator On |